# Architecture and data flow

## System overview

WeatherTool is a Scala backend, SolidJS frontend, and PostgreSQL database used to inspect Latvian weather observations and prepare map-based newsroom graphics.

```text
External providers                    Local/staging workflow
LVGMC station FTP/CSV ----+           Synthetic SQL seed
LVGMC forecast CSV -------+                    |
DMI HARMONIE APIs --------+                    v
                          v              PostgreSQL
                    Scala ingestion          |
                          |                   |
                          +---------> Scala/http4s API
                                             |
                                             v
                                      SolidJS web UI
                                             |
                                             v
                                 Canvas preview and PNG export
```

Staging currently exercises the PostgreSQL → API → frontend path with synthetic observations. It does not emulate LVGMC forecast files or HARMONIE GRIB files.

## Components

### Scala backend

- Serves JSON API routes and the built frontend from `web/dist`.
- Queries and aggregates station observations in PostgreSQL.
- Contains ingestion/parsing code for LVGMC station and forecast data.
- Contains HARMONIE discovery, download, GRIB parsing, and rendering support.
- Starts scheduled ingestion/cleanup tasks unless `ENABLE_SCHEDULED_JOBS=false`.

### SolidJS frontend

- Queries the backend using the same origin in production builds.
- Provides Stations, City Analysis, Faktiskā, Latvia overview, Database, HARMONIE, and LVGMC forecast workspaces. A separate Ūdens temperatūra production workspace is planned.
- Uses HTML canvas for broadcast maps and PNG export.
- Uses the bundled `ltv_meteo.otf` font for weather symbols; the glyphs are font characters, not emoji.

### PostgreSQL

- Stores normalized weather observations used by Stations, City Analysis, Faktiskā, and Latvia overview.
- Is accessible only inside the isolated Compose network in staging.
- Uses a bind-mounted `postgres/` runtime directory in the current Compose configuration.

## Main observation-data flow

1. An ingestion job parses provider station data, or the development seed inserts synthetic rows.
2. Observations are stored in the `weather` table.
3. The frontend requests an API route containing cities, time range, granularity, field, and aggregate key.
4. The backend performs the database query and returns JSON.
5. The frontend renders cards, lists, charts, or canvas graphics.
6. Broadcast maps can be downloaded as PNG files entirely in the browser.

## Broadcast-map flow

### City Analysis temperature maps

Queried city values are placed at predefined coordinates on one of four map backgrounds:

- `map_1920x1080`
- `map_1920x1080_wind`
- `map_3840x1440`
- `map_3840x1440_wind`

The operator can add title/source overlays and export the rendered canvas.

### Faktiskā

Faktiskā has a fixed 13-position station configuration. On page entry the frontend calls `/api/query/latest-temperatures/<cities>`. The backend selects the newest row per requested city and returns `tempAvg`, the station name, and its observation timestamp. The UI highlights missing or older observations and permits an explicit manual override without changing the stored observation.

Weather-font glyphs and wind values remain manual editorial inputs. One glyph can be applied to all fixed stations and exceptions changed individually. The browser composes these values on the fixed wind-template canvas and exports exactly 3840×1440 pixels. The production master images define the required output geometry; final Monda pixel-level comparison remains pending.

The glyph renderer measures each finished temperature badge, attaches the selected Daira glyph automatically, then applies a fixed optical correction shared by the Faktiskā template. The configuration also permits per-station offsets when later production comparison requires them. Operator input selects the symbol but never controls its coordinates.

### Ūdens temperatūra

Ūdens temperatūra is an independent fixed-template renderer. Its six ranges are currently manual editorial inputs rather than station-query results. A Latvian-named field configuration maps each water area to locked canvas coordinates. The workflow produces explicit 1920×1080 and 3840×1440 canvases and filenames; each size still requires comparison against newsroom output.

Monda Regular and Bold are bundled locally and used by the interface and generated text. Daira remains a separate font used only for weather-symbol glyphs.

## What the repository does not provide by itself

- Authorized provider accounts and credentials.
- Workplace deployment topology or authentication requirements.
- Real LVGMC forecast CSV fixtures for development.
- Real HARMONIE GRIB fixtures for development.
- A complete automated test suite.
- Production monitoring, backups, incident handling, or a reviewed security boundary.

See `UPDATE_ROADMAP.md` before considering workplace deployment.
